SUNLEO(__drivermansuffix__)

NAME
sunleo - Leo video driver

SYNOPSIS
Section "Device"
  Identifier "devname"
  Driver "sunleo"
  ...
EndSection
Section "Screen"
  ...
  Device "devname"
  ...
  DefaultDepth	32
  ...
EndSection

DESCRIPTION
leo is an __xservername__ driver for Sun Leo (ZX) video cards.

Also known as the ZX or T(urbo)ZX, Leo is a 24 bit accelerated 3D graphics card. Both cards are double-width, but the TZX also requires extra cooling in the form of an additional double-width fan card, so effectively takes up 4 SBus slots.

SUPPORTED HARDWARE
The leo driver supports all Sun stations that include a Leo chipset:

Workstations:

    Sun 4/15, 4/30, 4/75
    SPARCstation 5, 10, 20
    Ultra 1, 1E, 2

Servers:

    SPARCserver 1000,
    SPARCcenter 2000

CONFIGURATION DETAILS
You must set "DefaultDepth" to "32" in the Screen Section.
Please refer to __xconfigfile__(__filemansuffix__) for general configuration
details.  This section only covers configuration details specific to this
driver.

SEE ALSO
__xservername__(__appmansuffix__), __xconfigfile__(__filemansuffix__), xorgconfig(__appmansuffix__), Xserver(__appmansuffix__), X(__miscmansuffix__)

AUTHORS
Driver authors include: Jakub Jelinek <jakub@redhat.com>
Man page: Arnaud Quette <arnaud.quette@mgeups.com>