Main Page | Alphabetical List | Data Structures | File List | Data Fields | Globals

# usb-private.h

Go to the documentation of this file.

    00001 /* $XFree86$ */
    00002 /*
    00003  * Copyright 2002 Red Hat Inc., Durham, North Carolina.
    00004  *
    00005  * All Rights Reserved.
    00006  *
    00007  * Permission is hereby granted, free of charge, to any person obtaining
    00008  * a copy of this software and associated documentation files (the
    00009  * "Software"), to deal in the Software without restriction, including
    00010  * without limitation on the rights to use, copy, modify, merge,
    00011  * publish, distribute, sublicense, and/or sell copies of the Software,
    00012  * and to permit persons to whom the Software is furnished to do so,
    00013  * subject to the following conditions:
    00014  *
    00015  * The above copyright notice and this permission notice (including the
    00016  * next paragraph) shall be included in all copies or substantial
    00017  * portions of the Software.
    00018  *
    00019  * THE SOFTWARE IS PROVIDED "AS IS", WITHOUT WARRANTY OF ANY KIND,
    00020  * EXPRESS OR IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES OF
    00021  * MERCHANTABILITY, FITNESS FOR A PARTICULAR PURPOSE AND
    00022  * NON-INFRINGEMENT.  IN NO EVENT SHALL RED HAT AND/OR THEIR SUPPLIERS
    00023  * BE LIABLE FOR ANY CLAIM, DAMAGES OR OTHER LIABILITY, WHETHER IN AN
    00024  * ACTION OF CONTRACT, TORT OR OTHERWISE, ARISING FROM, OUT OF OR IN
    00025  * CONNECTION WITH THE SOFTWARE OR THE USE OR OTHER DEALINGS IN THE
    00026  * SOFTWARE.
    00027  */
    00028
    00029 /*
    00030  * Authors:
    00031  *   Rickard E. (Rik) Faith <faith@redhat.com>
    00032  *
    00033  */
    00034
    00041 #ifndef _USB_PRIVATE_H_
    00042 #define _USB_PRIVATE_H_
    00043
    00044 #include "dmxinputinit.h"
    00045 #include "inputstr.h"
    00046 #include "Xos.h"
    00047 #include <errno.h>
    00048 #include <linux/input.h>
    00049 #include "usb-common.h"
    00050
    00051                                 /*  Support for force feedback was
    00052                                  *  introduced in Linxu 2.4.10 */
    00053 #ifndef EV_MSC
    00054 #define EV_MSC      0x04
    00055 #endif
    00056 #ifndef EV_FF
    00057 #define EV_FF       0x15
    00058 #endif
    00059 #ifndef LED_SLEEP
    00060 #define LED_SLEEP   0x05
    00061 #endif
    00062 #ifndef LED_SUSPEND
    00063 #define LED_SUSPEND 0x06
    00064 #endif
    00065 #ifndef LED_MUTE
    00066 #define LED_MUTE    0x07
    00067 #endif
    00068 #ifndef LED_MISC
    00069 #define LED_MISC    0x08
    00070 #endif
    00071 #ifndef BTN_DEAD
    00072 #define BTN_DEAD    0x12f
    00073 #endif
    00074 #ifndef BTN_THUMBL
    00075 #define BTN_THUMBL  0x13d
    00076 #endif
    00077 #ifndef BTN_THUMBR
    00078 #define BTN_THUMBR  0x13e
    00079 #endif
    00080 #ifndef MSC_SERIAL
    00081 #define MSC_SERIAL  0x00
    00082 #endif
    00083 #ifndef MSC_MAX
    00084 #define MSC_MAX     0x07
    00085 #endif
    00086
    00087                                 /* Support for older kernels. */
    00088 #ifndef ABS_WHEEL
    00089 #define ABS_WHEEL   0x08
    00090 #endif
    00091 #ifndef ABS_GAS
    00092 #define ABS_GAS     0x09
    00093 #endif
    00094 #ifndef ABS_BRAKE
    00095 #define ABS_BRAKE   0x0a
    00096 #endif
    00097
    00098 #define NUM_STATE_ENTRIES (256/32)
    00099
    00100 /* Private area for USB devices. */
    00101 typedef struct _myPrivate {
    00102     DeviceIntPtr   pDevice;
    00103     int            fd;
    00104     unsigned char  mask[EV_MAX/8 + 1];
    00105     int            numRel, numAbs, numLeds;
    00106     int            relmap[DMX_MAX_AXES];
    00107     int            absmap[DMX_MAX_AXES];
    00109     CARD32         kbdState[NUM_STATE_ENTRIES];
    00110     DeviceIntPtr   pKeyboard;
    00112     int            pitch;
    00113     unsigned long  duration;
    00115     /* FIXME: dmxInput is never initialized */
    00116     DMXInputInfo   *dmxInput;
    00117 } myPrivate;
    00118 #endif