I128(__drivermansuffix__)

NAME
i128 - Number 9 I128 video driver

SYNOPSIS
Section "Device"
  Identifier "devname"
  Driver "i128"
  ...
EndSection

DESCRIPTION
i128 is an __xservername__ driver for Number 9 I128 video cards. The driver is accelerated and provides support for all versions of the I128 chip family, including the SGI flatpanel configuration. Multi-head configurations are supported.

SUPPORTED HARDWARE
The i128 driver supports PCI and AGP video cards based on the following I128 chips:

I128 rev 1
    (original)

I128-II

I128-T2R
    Ticket 2 Ride

I128-T2R4
    Ticket 2 Ride IV

CONFIGURATION DETAILS
Please refer to __xconfigfile__(__filemansuffix__) for general configuration details. This section only covers configuration details specific to this driver.

The driver auto-detects the chipset type and may not be overridden.

The driver auto-detects the amount of video memory present for all chips and may not be overridden.

The following driver Options are supported:

Option "HWCursor" "boolean"
    Enable or disable the HW cursor. Default: on.

Option "NoAccel" "boolean"
    Disable or enable acceleration. Default: acceleration is enabled.

Option "SyncOnGreen" "boolean"
    Enable or disable combining the sync signals with the green signal. Default: off.

Option "Dac6Bit" "boolean"
    Reduce DAC operations to 6 bits. Default: false.

Option "Debug" "boolean"
    This turns on verbose debug information from the driver. Default: off.

SEE ALSO
__xservername__(__appmansuffix__), __xconfigfile__(__filemansuffix__), xorgconfig(__appmansuffix__), Xserver(__appmansuffix__), X(__miscmansuffix__)

AUTHORS
Authors include: Robin Cutshaw (driver), Galen Brooks (flatpanel support).