/* $XFree86: xc/programs/Xserver/hw/xfree86/drivers/nsc/gfx/release.txt,v 1.1 2002/12/10 15:12:27 alanh Exp $ */
Durango Release Notes
Version 2.49.01
Win98/WinXP/DOS/Linux
January 29, 2003

-----------------------------------------------------------------------------
PRODUCT INFORMATION
-----------------------------------------------------------------------------
Durango is a graphics/video software support package designed to assist in the
development of display drivers and embedded applications. The core of this 
package is source code that performs most of the graphics related 
functionality for the National Semiconductor ® Geode family of products.  
Development time for new software is reduced by using these routines to access
the hardware.

-----------------------------------------------------------------------------
INSTALLATION INSTRUCTIONS
-----------------------------------------------------------------------------
Download the file to a directory.  Modify and include the file durango.c 
according to the needs of the application. 

-----------------------------------------------------------------------------
REVISION HISTORY
-----------------------------------------------------------------------------

02/05/03 Version 2.49.02

-----------------------------------------------------------------------------
FUNCTIONAL CHANGES
-----------------------------------------------------------------------------

* Fixed GX2 left clipping for 4:2:0 video.

=============================================================================

01/29/03 Version 2.49.01

-----------------------------------------------------------------------------
FUNCTIONAL CHANGES
-----------------------------------------------------------------------------

* Removed unused variable in CS5530 video code.
* Changed max supported pixel clock for SCx2xx to 157.5 MHz.

=============================================================================

01/10/03 Version 2.49.00

-----------------------------------------------------------------------------
FUNCTIONAL CHANGES
-----------------------------------------------------------------------------

* Added extra wait loop when polling for CRC completion.
* Removed code that sets the pitch offsets for 4:2:0 video within
  gfx_set_video_size.
* Fixed panning code to work with any display pitch.
* Added code to clear the PLL bypass bit when setting the dot PLL.
* Fixed panning code so cursor never disappears when panning.
* Changed GX2 delay loops to do a volatile register read to prevent
  the entire delay loop from being discarded by a compiler.

=============================================================================

11/19/02 Version 2.47.00

-----------------------------------------------------------------------------
FUNCTIONAL CHANGES
-----------------------------------------------------------------------------

* Updated gfx2_* routines to use a signed stride.
* SW workaround for issue #134.8 - Strange horizontal lines appearing while
  drawing lines.
* Implemented gfx_set_video_left_crop for CS5530
* Updated sub carrier reset values for NTSC and PAL.

=============================================================================

08/29/02 Version 2.45.00

-----------------------------------------------------------------------------
FUNCTIONAL CHANGES
-----------------------------------------------------------------------------

* Modified gfx_set_cursor_position to use cursor position when panning and not adjust
  using hotspots.
* Added new routine gfx_get_refreshrate_from_mode.
* Added gfx_text_blt routine.
* Added gfx_get_tv_display_mode_frequency routine.
* Added gfx_get_frequency_from_refreshrate routine.
* Added gfx_set_video_cursor_enable routine.
* Fixed Linux compilation warnings.
* Updated modeset code to clear panning variables.
* Added panel timings for 1600x1200 desktops.
* Removed wait for VBlank when panning using cursor routines.

=============================================================================

07/12/02 Version 2.43.03

-----------------------------------------------------------------------------
FUNCTIONAL CHANGES
-----------------------------------------------------------------------------

* Modified gfx_get_display_mode to support 56 Hz modes.
* Added support for 8K pitch when setting a true color mode above 1024x768
* Added a byte-packed option to gfx2_mono_expand_blt
* Fix for Carmel D2 alpha blending issue.
* Added typecasts for proper compilation.
* Fixed CS5535 MBIU address.
* Added new GX2 routine, gfx2_text_blt
* Added MSR implementations for Linux.
* Further optimized default GX1 string macros.
* Added new routine, gfx_set_panel_present to allow panning without adjusting panel timings.
* Added assembly macros for 32-bit Windows applications.

=============================================================================

03/21/02 Version 2.41.02

-----------------------------------------------------------------------------
FUNCTIONAL CHANGES
-----------------------------------------------------------------------------

* Optimized GX2 Bitmap-to-screen BLTs by using a 2-line offscreen scratch area.
* Fixed a bug in GX2 monochrome bitmap BLTs.
* Fixed gfx_get_clock_frequency for GX2 2.0
* Added 56 Hz support to gfx_get_clock_frequency
* Changed gfx_set_compression_size to subtract header size
* Changed gfx_get_compression_size to add header size

=============================================================================

03/04/02 Version 2.39.01

-----------------------------------------------------------------------------
FUNCTIONAL CHANGES
-----------------------------------------------------------------------------

* Added support for CS5535 MSRs.
* Fixed a bug in monochrome bitmap BLTs.
* Added support for 32-bit CRC mechanism in GX2 2.0.
* First official GX2 release.
* Added support for new Dot PLL mechanism in GX2 2.0
* Added support for Carmel D1.1 and D2.

=============================================================================

01/24/02 Version 2.37.00

-----------------------------------------------------------------------------
FUNCTIONAL CHANGES
-----------------------------------------------------------------------------

* Changed gfx_get_clock_frequency, gfx_get_cursor_offset and gfx_get_display_offset
  to be outside the GFX_READ_ROUTINES flag.
* Modified the modeset code to set higher FIFO priority levels for high bandwidth
  modes.
* Init code no longer returns Redcloud ID when no chip detected.
* Added fix for Redcloud 1.x rev ID
* New GX2 PLL settings - updates to the 14 MHz table and a new 48 MHz table.
* Optimized all bitmap-to-screen routines.  Optimizations include new macros that
  allow correct operation in a 16-bit environment.
* 3K cache is now assumed to be the default scratchpad configuration.
* gfx_get_frame_buffer_size for GX2 no longer uses a VGA register.  This allows
  correct operation even with an external VGA card present in the system.
* Added support for 1152x864 desktop resolution on a flat panel.
* Added 24BPP support for large display modes.
* Modified gfx_set_video_scale such that an identity scale is now default.
* Modifed flat panel modeset code to dynamically determine the size of the mode table.
* Added support for Carmel Rev D2.

=============================================================================

10/22/01 Version 2.35.01

-----------------------------------------------------------------------------
FUNCTIONAL CHANGES
-----------------------------------------------------------------------------

* New release notes format.
* Added fix for SC1200 issue #813 (TVOut field indication is reversed.
* Added check for invalid values in video upscale.
* Fixed compilation warnings and run-time errors under DOS.
* Added new macros for word I/O.
* Optimized VSAII MSR code to used DWORD I/O.
* Fixed SoftVG base PCI base addresses.
* Several fixes to Redcloud API found during bringup.
* Modified Durango to support 4-pixel video alignment for Redcloud.
* Added the functions gfx_test_vip_overflow, gfx_get_vip_line,
  gfx_set_decoder_luminance_filter, gfx_set_tv_YV_delya and 
  gfx_set_tv_field_status_invert.
* Added support for Carmel D1 revision ID.
* Moved gfx_get_vip_base and gfx_get_vbi_pitch outside of the 
  GXF_READ_ROUTINES flag.
* Minor fixes to saa7114.c and gfx_set_tv-enable.
* Added don't care option in gfx_set_vip_base.
* Added fix for SC1200 issue #1121 (VIP FIFO bus request threshold bit 
  is inverted.

=============================================================================

07/31/01 Version 2.33.02

-----------------------------------------------------------------------------
FUNCTIONAL CHANGES
-----------------------------------------------------------------------------
* Completed implementation of vertical downscaling support for GX2.
* Added a method to lock the display controller timings.
* Added support for SC1200 Rev C.
* Small modifications to gfx_set_video_format.
* Removed unused and unimplemented I2C functions.
* Changes to prevent errors and compiler warnings in DOS.
* Updated headers to include both BSD and GPL licenses.

=============================================================================

06/08/01 Version 2.31.00

-----------------------------------------------------------------------------
FUNCTIONAL CHANGES
-----------------------------------------------------------------------------
* Added new routines to manipulate vertical video downscaling on GX2.
* Minor fixes to the function gfx_read_window_crc.
* Implemented all init routines for GX2 except gfx_get_core_freq.
* Added support for 27MHz reference frequency to the GX2 PLL.
* Added new function gfx_get_softvga_active.
* Minor changes to the function sc1200_reset_video.
* Fixed some minor compiler warnings.

=============================================================================

04/25/01 Version 2.29.00

-----------------------------------------------------------------------------
FUNCTIONAL CHANGES
-----------------------------------------------------------------------------
* Disabled all CSC when setting an RGB video format.
* Modified sc1200_set_video_size to add 2 to the window height.
* Modified code to support the accelerator and cursor in pixel and line double modes.
* Modified gfx_get_core_freq to be a dynamic API routine.
* Added the function gfx_read_window_crc for GX2.
* Added init routine gfx_get_graphics_register_base for GX2.
* Added new macros to access the scratchpad RAM to support Win2K and WinME.
* Added mew macros to access the GP registers for GX2.

=============================================================================

04/06/01 Version 2.27.00

-----------------------------------------------------------------------------
FUNCTIONAL CHANGES
-----------------------------------------------------------------------------
* Added new TV read functions:
     gfx_get_tv_enable, gfx_get_tv_output, gfx_get_tv_display_mode,
     gfx_get_tv_mode_count, gfx_is_tv_display_mode_supported
* Added new function gfx_set_display_bpp.
* Added new function gfx_get_frame_buffer_line_size.
* Modified gfx_set_vbi_base to accept pure physical addresses instead of offsets.
* Implemented video and display controller routines for GX2.
* Modified some initialization routines to be dynamic.
* Created new API extension for GX2 MSR accesses.
* Added new icon routines for GX2.
* Modified gfx_set_tv_display to preserve current bpp.
* Minor modifications to gfx_set_tv_format, gfx_set_video_palette and 
  gfx_set_video_palette entry.
* Added support for 1152x864@75Hz

=============================================================================

03/12/01 Version 2.25.00

-----------------------------------------------------------------------------
FUNCTIONAL CHANGES
-----------------------------------------------------------------------------
* Adapted new revision format system.
* Synchronized with NSTA Durango.  Updated support for all SC1200 features.
* Added support for 640x400 as well as emulated VGA modes.
* Added new routines to access single palette color entries.
* Added new routine to return the maximum supported pixel clock.
* Added new routine gfx_set_crt_enable to manipulate the CRT display logic.
* Added new rendering routine gfx_color_pattern_fill.
* Added 4:2:0 and RGB video format support for CS5530 and SC1200.
* Modified code to allow operation under DOS.

=============================================================================

07/21/00 Version 2.04

-----------------------------------------------------------------------------
FUNCTIONAL CHANGES
-----------------------------------------------------------------------------
* Verified Xfree86 driver version 1.1.4 under Linux, and ce v2.3.
* Merged sc1200 changes.
* Added routines to support the query of current display mode.
* Added functions gfx_enable_softvga, dfx_disable_softvga. 
* Added code optimization in rendering loops to use 32 bit writes where possible.
* Added gfx_is_mode_supported to query if given mode supported by the h/w.
* Added Flat panel support, realy testing with panel done only for 800x600.
* Removed subtraction of 16 from gfx_set_compression_size.
* Added version.h file to reflect the version of the durango used. 

=============================================================================

03/03/00 Version 2.01

-----------------------------------------------------------------------------
FUNCTIONAL CHANGES
-----------------------------------------------------------------------------
* Verified Xfree86 driver version 1.1 under FreeBSD and Linux.
* Added automatic detection of BLT buffer bases in "gfx_set_bpp" routine.
* Fixed improper setting of VGA attrubute controller index register.
* Moved "gfx_get_display_bpp" to always be included.
* Moved "gfx_get_hactive" and "gfx_get_vactive" to always be included.
* Clipped video source size if off bottom or right side.
* Properly adjusted video offset if clipped on the top side.
* Added "gfx_get_video_line_size" and "gfx_get_video_xclip" routines.

=============================================================================

02/21/00 Version 2.00

-----------------------------------------------------------------------------
FUNCTIONAL CHANGES
-----------------------------------------------------------------------------
* Added gfx_vga.c.
* Added write to GP_BLIT_STATUS in "gfx_set_bpp" routine.
* Verified alpha blending on SC1200.
* Removed "gfx_set_blt_buffers" routine.

=============================================================================

02/09/00 Version 1.20

-----------------------------------------------------------------------------
FUNCTIONAL CHANGES
-----------------------------------------------------------------------------
* Verified display modes and graphics rendering on SC1200.
* Updated PLL table for SC1200 to set modes.
* DURANGO.C FILE CHANGE!: Modifed and added compiler definitions.
* Split gfx_disp.c file into gu1_disp.c and gu2_disp.c
* Split gfx_rndr.c file into gu1_rndr.c and gu2_rndr.c
* Split gfx_vid.c file into vid_5530.c, vid_1400.c, and vid_1200.c
* Split gfx_vip.c file into vip_1400.c and vip_1200.c
* Split gfx_tv.c file into geode_tv.c and fs451_tv.c
* Split gfx_i2c.c file into acc_i2c.c and gpio_i2c.c.
* Split gfx_dcdr.c file to saa7114.c 
* Added GFX_READ_ROUTINES compiler definition.  
* Moved routines from gfx_read.c (no longer exists) to other files.
* Abstracted display controller access in the video overlay routines.
* Added routines to control display compression hardware.

=============================================================================

01/28/00 Version 1.13

-----------------------------------------------------------------------------
FUNCTIONAL CHANGES
-----------------------------------------------------------------------------
* Passes randomly generated rendering tests in Darwin for GXLV.
* Fixed bug for large bitmap to screen BLTs (greater than 64K).
* Fixed bug for pattern fills using solid source data for plane masks.

=============================================================================

01/14/00 Version 1.12

-----------------------------------------------------------------------------
FUNCTIONAL CHANGES
-----------------------------------------------------------------------------
* Added proper use of hotspot to gfx_set_cursor_position.
* Fixed buffer size to handle all frame buffer start address alignments.
* Added initial version of gfx_tv.c.

=============================================================================

01/07/00 Version 1.11

-----------------------------------------------------------------------------
FUNCTIONAL CHANGES
-----------------------------------------------------------------------------
* Fixed bug with transparent BLTs (loading transparent color into BB1).
* Added definition of gfx_color_bitmap_to_screen_blt to gfx_rtns.h.
* Added gfx_color_bitmap_to_screen_xblt (transparent bitmap to screen).

=============================================================================

12/21/99 Version 1.10

-----------------------------------------------------------------------------
FUNCTIONAL CHANGES
-----------------------------------------------------------------------------
* Added additional video decoder routines to gfx_dcdr.c.
* Added VBI routines to gfx_vip.c.
* Added alpha blending routines for SC1200 to gfx_vid.c

=============================================================================

10/01/99 Version 1.00

-----------------------------------------------------------------------------
FUNCTIONAL CHANGES
-----------------------------------------------------------------------------
* Added video port, video decoder, I2C, and hardware query rouines.
* New files: gfx_vip.c, gfx_dcdr.c, gfx_i2c.c, gfx_read.c.

=============================================================================

08/27/99 Version 0.05

-----------------------------------------------------------------------------
FUNCTIONAL CHANGES
-----------------------------------------------------------------------------
* INTERFACE CHANGE: Changed "gfx_csptr[]" to "gfx_vidptr" and "gfx_vipptr".
* Added "gfx_get_vid_register_base" and "gfx_get_vip_register_base".
* Added initial PLL table for SC1400.
* Verified mode set and video overlay routines work correctly on SC1400.
* Updated initilization routines.
* Added update of graphics engine in "gfx_set_display_pitch".

=============================================================================

08/20/99 Version 0.04

-----------------------------------------------------------------------------
FUNCTIONAL CHANGES
-----------------------------------------------------------------------------
* INTERFACE CHANGE: "gfx_load_*" routines changed to "gfx_set_*" for naming
  consistency.  The "gfx_text_glyph" routine was removed. 
* Added video overlay routines.
* Added gfx_vid.c file.

=============================================================================

08/16/99 Version 0.03

-----------------------------------------------------------------------------
FUNCTIONAL CHANGES
-----------------------------------------------------------------------------
* INTERFACE CHANGE: Access to CS5530 now through separate pointer.  Project 
  must declare and map the gfx_csptr[GFX_CSPTR_SIZE] variable.
* Added durango.c file as template for main source file.
* Added gfx_init.c file.

=============================================================================

08/04/99 Version 0.02

-----------------------------------------------------------------------------
FUNCTIONAL CHANGES
-----------------------------------------------------------------------------
* Additional modes in gfx_mode.h file.
* Separated register definitions from gfx_defs.h into gfx_regs.h.

=============================================================================

07/30/99 Version 0.01

-----------------------------------------------------------------------------
FUNCTIONAL CHANGES
-----------------------------------------------------------------------------
* Initial release.
-----------------------------------------------------------------------------

