VESA(__drivermansuffix__)

NAME
vesa - Generic VESA video driver

SYNOPSIS
Section "Device"
  Identifier "devname"
  Driver "vesa"
  ...
EndSection

DESCRIPTION
vesa is an __xservername__ driver for generic VESA video cards. It can drive most VESA-compatible video cards, but only makes use of the basic standard VESA core that is common to these cards. The driver supports depths 8, 15 16 and 24.

SUPPORTED HARDWARE
The vesa driver supports most VESA-compatible video cards. There are some known exceptions, and those should be listed here.

CONFIGURATION DETAILS
Please refer to __xconfigfile__(__filemansuffix__) for general configuration details. This section only covers configuration details specific to this driver.

The driver auto-detects the presence of VESA-compatible hardware. The ChipSet name may optionally be specified in the config file "Device" section, and will override the auto-detection:

    "vesa"

The following driver Options are supported:

Option "ShadowFB" "boolean"
    Enable or disable use of the shadow framebuffer layer. Default: on. This option is recommended for performance reasons.

SEE ALSO
__xservername__(__appmansuffix__), __xconfigfile__(__filemansuffix__), xorgcfg(__appmansuffix__), xorgconfig(__appmansuffix__), Xserver(__appmansuffix__), X(__miscmansuffix__)

AUTHORS
Authors include: Paulo Ce'sar Pereira de Andrade.